
DeConvEELS plug-in for Gatan DigitalMicrograph
--------------------------------------------------------------------------------

Version 4.0
January 2026

--------------------------------------------------------------------------------
Contact

General enquiries on the DeConvEELS for DigitalMicrograph should be sent to: 
HREM Research Inc.
14-48 Matsukazedai
Higashimatsuyama 
Saitama 355-0055
Japan

Phone: +81 493 35 3913
Fax: +81 493 35 3919
email: mailto:support@hremresearch.com
Website: http://www.hremresearch.com /

--------------------------------------------------------------------------------
Files
	- DeConvEELS64.gtk: main compiled script file
	- DeConvEELS64.dll: dll file
	- DeConvBasicLib64.gtk: support compiled script file
	- DeConvEELS.pdf: help file
	- ReadMe.txt: this file

--------------------------------------------------------------------------------
Installation
	Installation is straightforward. Just copy the files to the following folders.
	Go to \Gatan\Plugins folder: DeConvEELS64.gtk, DeConvEELS64.dll, DeConvBasicLib64.gtk
	Go to \Gatan\Help folder: DeConvEELS.pdf
	
[NOTE] These Gatan folders may be found at two places, namely in "Program files" and/or "ProgramData" 
of Windows 7.  Since the Program files folder is no longer accessible to regular users, Gatan 
recommends to use the latter ProgramData folder to install the plug-in and help files. 
	
[NOTE] IPU plug-in should be also installed to run this plug-in.

--------------------------------------------------------------------------------
Release Notes
4.0   New command for continue and show log are added.
3.6.1 Extended capability of SI_RichardsonLucy command 
3.6   DLL optimization for GMS 2.x by using INTEL C++ Compiler
3.5   New command for the Process Area; Log data (ResultLog etc) will be concatenated.
3.4   Some bug fixes
3.3.2 Windows 8 supported by a 64bit version
3.3.1 Bug fix for the smoothing width and some minor modifications
3.3   Add 'Adjust spectrum length' and some bug fix from v3.1 (add the calibration etc.)
3.2   Update for GMS 2.3
3.1   GMS2.0 Support
3.0   Can handle an image of any size (including non-sauare image)
      Performnce improvement and modified to work with IPU plug-ins
      Support a range ROI to specify the interest area of the spectrum
